2 | Installation of TAPI 120

2.1 | General

Scope of installation

The components to be installed for TAPI 120 can be selected when during setup. The following components are available in principle:

• | TSP

• | CMD

Installation and configuration

If both components are selected for installation, the individual installation routines and dialogs for entering the configuration parameters may be automatically started one after the other. In the present document, installation procedures are described in section Starting installation and configurable parameters are described in section Configuring components.