2.2.1 | Installing the CMD component

Different confirmation prompts might appear during TAPI 120 configuration.

If required the CMD component can be installed on a central PC. This PC has to meet the following requirements:

• | Cover the operating time of all HiPath TAPI 120 clients.

• | It is not allowed to use applications that might cause a resource supply shortfall (CPU load, network traffic, etc.).

1. | A welcome dialog is not displayed when installing the CMD component. Progress is displayed in a window.

2. | For PCs with two network cards, a dialog appears prompting you to select the IP address to be used.

3. | The CMD configuration dialog opens automatically following successful CMD installation. The required parameters can be entered in this dialog or configured at a later stage.

Display

| The individual configuration parameters are described under Configuring the CMD component.

CMD installation is complete once you have exited the configuration dialog. The component TSP may now be installed automatically depending on the setup type selected.