1.2 | Requirements

Requirements for server connection

Connection to the communication systems or connection to CMD is realized via TCP/IP.

Software requirements for TAPI 120 PCs

• | 32-bit operation system versions:

| - | Windows 8.1 / 8 (except RT Version)

| - | or Windows 7 (except Starter / Home Basic / Home Premium Edition)

| - | or Windows Vista (except Home Edition)

| - | or Windows Server 2008

• | 64-bit operation system versions:

| - | Windows 8.1 / 8 (except RT Version)

| - | or Windows 7 (except Starter / Home Basic / Home Premium Edition)

| - | or Windows Server 2012 / Windows Server 2012 R2

| - | or Windows Server 2008 / Windows Server 2008 R2

Different confirmation prompts might appear during TAPI 120 configuration.

For more information about appropriate operating system variants please consider the file readme.txt on the TAPI 120 installation CD.

TAPI 120 configurations with 64-bit operation system versions

Possible configurations for TAPI 120 on 64-bit operation system versions are:

• | TAPI 120 with direct connection:

| - | PC with 64-bit operation system version with the 64-bit version of TAPI 120 and 32-bit or 64-bit TAPI applications

• | TAPI 120 with connection via CMD

| - | PC with 64-bit operation system version with the 64-bit version of CMD

| - | Client-PC with 64-bit operation system version with the 64-bit version of TAPI 120 and 32-bit or 64-bit TAPI applications

Other requirements

• | Network protocol: TCP/IP must be installed and configured.

• | Installation of TAPI 120 must be executed by an user with administration rights.

Overview of used TAPI 120 ports (default)

Port number
Description
7001
CSTA-link th the system (HiPath 500 / OpenOffice EE / 2000 / 3000)
8001
CSTA-link to CMD
8800
CSTA-Link to OpenScape Office

Limitations

Operating TAPI 120 and TAPI 170 on the same PC is not possible.