3.2.5 | CMD parameters for CTI firewall

Every TAPI 120 client that is connected to the CMD and permitted to seize a line, must be entered in the CTI Firewall tab to enable this access.

> | Activate the CTI Firewall tab in the CMD configuration dialog.

| You will see a list of the TAPI 120 clients (IP addresses) already configured for access:

Display

| Entries are displayed with the following information:

Column
Description
Name
Freely chosen name for the TAPI 120 client, enabling a single entry in the firewall to be identified.
Call number
Call number of the extension to be monitored
TAPI 120 IP addresses
IP address of the TAPI 120 client

Sorting the list displayed

The list can be sorted in ascending/descending order according to column content by clicking the relevant column heading, e.g. Name.

Saving parameters

> | To save entries, click Apply (to configure parameters in other tabs for example) or OK (to exit the configuration dialog and save changes).
> | A confirmation message appears in both cases before the parameter values are saved in the database. Click Yes to confirm this message.

3.2.5.1 | Editing/deleting an entry

Editing an entry

> | To edit the parameters of an entered TAPI 120 client, double-click the corresponding value. The value can then be changed in the entry field displayed.

Deleting an entry

> | Highlight the entry to be deleted using the mouse and click Delete or press the key. The entry is then deleted from the list.

3.2.5.2 | Adding a TAPI 120 client

1. | Click Add in the CTI Firewall tab.

2. | Enter the data of the TAPI 120 client in the input dialog and confirm with OK. You return to the CTI Firewall tab.

An unlimited number of clients can be entered on this tab. However, please note that the number of clients permitted to seize lines at any one time is limited by the licensing agreement (see also CMD license parameters).