3.3.2 | Configuration of TSP 120 parameters

The configuration dialog appears following installation or manual activation:

Display for CMD

Display for HiPath 500

Display for HiPath OpenOffice EE

Display for HiPath 2000

Display for HiPath 3000

Display for OpenScape Office

| The parameters contain the following information:

Parameter
Description
System
For selecting the connected system. The following baud rates can be selected:
| - | CMD
| - | HiPath 500
| - | HiPath OpenOffice EE
| - | HiPath 2000
| - | HiPath 3000 (default)
| - | OpenScape Office
CSTA link
Connection type between TSP and the system. By default this is always TCP/IP and cannot be changed.
Call number Name
Enter the Call number of the telephone and Name of the telephone's user.
IP address
With system connection via TCP/IP this is the system's IP address determined during installation and configuration of the system.
IP port
Connecting the system without CMD you enter the IP port number of the system determined during its installation and configuration (7001).
Connecting the system with CMD you enter the listener port number of the CMD determined by the CMD configuration, e.g. 8001.
Trunk access code start
Trunk access code end
Range of system station numbers for trunk access codes. The values may need to be aligned with the deviating system settings. An entry is mandatory. The default values are:
• | HiPath 500: 801 / 816
• | HiPath 2000: 7801 / 7840
• | HiPath OpenOffice EE: 7801 / 7840
• | HiPath 3000: 7801 / 7920
• | OpenScape Office: ##700 / ##949
Trace
Option for activating trace messages (CSTA messages) that can be interpreted using separate standard debugging tools.

Saving parameters

> | To save entries, click Apply (to configure parameters in other tabs for example) or OK (to exit the configuration dialog and save changes).
> | A confirmation message appears in both cases before the parameter values are saved in the registration database. Click Yes to confirm this message.

It is necessary to restart the TSP (net stop tapisrv), for instance after modifying the connection type (CSTA link).

Importing / exporting of TSP configuration parameters

Exporting
1. | The configured general configuration parameters can be exported to a file, e.g. to save a specific level. Click Config Export to start exporting.
2. | Enter the name of the export file in the dialog displayed and confirm.
| The entries are exported. The TSP configuration dialog re-appears.
Importing
1. | General configuration parameters can also be imported from a file, e.g. containing exported parameter information. Click Config Import to start importing.
2. | Select the file to be imported.
| The entries are imported and the TSP configuration dialog re-appears.